{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cálculo de datos previos","Ficha resumen","Hoja3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cálculo de datos previos","index":0,"n_rows":12,"n_cols":3,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Suma de precios unitarios"]
[null,"Precio unitario del consumo de energía (PU_ENERGIA)",0.34560000000000002]
[null,"Precio unitario de la electrificación rural (PU_ELECTRORURAL)",7.4000000000000003E-3]
[null,null,{"$f":"SUM(C4:C5)","v":0.35300000000000004}]
[]
[null,"Suma de costos fijos"]
[null,"Cargo fijo",2.41]
[null,"Mantenimiento y reposición de conexión",1.01]
[null,"Alumbrado público",4.08]
[null,null,{"$f":"SUM(C9:C11)","v":7.5}]

{"sheet":"Ficha resumen","index":1,"n_rows":7,"n_cols":5,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Datos para el cálculo final","Valor","Unidades"]
[null,"Potencia de un electrodoméstico",290,"W","Aparece en los DATOS DE PLACA (etiqueta) del equipo"]
[null,"Número de horas al mes",30,"horas por mes"]
[null,"Suma de precios unitarios (consumo de energía, electrificación rural)",0.35300000000000004,"S/.","Valor calculado en la hoja \"Cálculo de datos previos\""]
[null,"Costos fijos (Cargo fijo, mantenimiento,alumbrado público)",7.5,"S/.","Valor calculado en la hoja \"Cálculo de datos previos\""]
[null,"COSTO TOTAL PARA EL ELECTRODOMÉSTICO ELEGIDO",{"$f":"Calc_costoenergia(C3,C4,C5,C6)","v":12.1371},"S/."]

{"sheet":"Hoja3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}