{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["INCREMENTO EN TRATAMIENTO"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"INCREMENTO EN TRATAMIENTO","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[[10,0,10,2],[1,5,1,9],[2,0,2,1],[0,0,0,6],[16,0,16,2],[18,0,18,2],[19,0,19,2],[3,0,3,1],[11,0,11,2],[12,0,12,2],[13,0,13,2],[14,0,14,2],[6,0,6,4],[7,0,7,4],[9,0,9,2]]}
["TAMAÑO DE PARTICULAS DE MINERAL EN EL ALIMENTO Y EN EL PRODUCTO"]
[]
["Tamaño del min. alim.   =",null,12700,"micrones  =","F80"]
["Tamaño del min. Prod.   =",null,75,"micrones  =","P80"]
["Peso específico min.     =",null,2.8]
[]
["CALCULO DEL CONSUMO DE ENERGIA POR TONELADA  DE"]
["MINERAL TRATADO"]
[]
["Voltaje suministrado al motor            =",null,null,2300,"V"]
["Se toma de la placa"]
["Amperaje suministrado al motor        =",null,null,45,"A"]
["Promedio de las tres líneas",null,null,{"$f":"IF(F13>0,\"Incrementar Tratamiento\",\"Tener cuidado\")","v":"Tener cuidado"}]
["Factor de corrección                       =",null,null,{"$f":"3^(0.5)","v":1.7320508075688772}]
["En estrella del motor trifásico"]
["Factor de potencia                          =",null,null,0.8]
["Factor de conversión de W a Kw      =",null,null,1000]
["Tonelaje de mineral alimentado        =",null,null,300,"día     =",{"$f":"+D18/24","v":12.5},"hr"]
["Consumo de energía                        =",null,null,{"$f":"+(D10*D12*D14*D16)/D17","v":143.41380686670306},"Kw      =",{"$f":"D19/0.746","v":192.24370893659926},"HP"]
["Energía realmente suministrada        =",null,null,{"$f":"+D19/(F18)","v":11.473104549336245},"Kw-h / TC"]
["Indice de trabajo Wi   =",null,null,{"$f":"(D20)/((10/(C4^0.5)-10/(C3^0.5)))","v":10.76311676355046},"Kw-h / TC"]
[]
["Potencia Insatlada HP =",null,400,"HP"]
["La potencia instalada es de 400 HP, con lo cual se puede calcular la capacidad máxima,-"]
["asumiendo que los alimentos y productos mantienen sus caracteísticas granulométricas."]
[]
["Capacidad Máxima CM =",null,{"$f":"(C23*0.746/D20)","v":26.00865343088531},"TCSPH"]
[{"$f":"IF(C28>0,\"Incrementar Tratamiento\",\"Tener cuidado\")","v":"Incrementar Tratamiento"},null,{"$f":"+C27-F18","v":13.50865343088531},"TCSPH   =",{"$f":"+C28*24","v":324.20768234124745},"TCSPD"]