{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Hoja1","Hoja2","Hoja3"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Hoja1","index":0,"n_rows":23,"n_cols":3,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
["MODELO","ALTURA","CONSIDERACIONES"]
["D8T",2000,"pedir repuestos"]
["938H",3000,"pedir repuestos"]
["D6T",4000,"pedir repuestos"]
["140K",1200,"No considerar"]
["140K",1600,"pedir repuestos"]
["324DL",4000,"pedir repuestos"]
["966H",3000,"pedir repuestos"]
["336DL",1500,"No considerar"]
["CS533E",4800,"pedir repuestos"]
["CS533E",1700,"pedir repuestos"]
["140K"]
["336DL"]
["336DL"]
["CS533E"]
["329DL"]
["962H"]
["962H"]
["D8T"]
["Ejemplo:"]
["Si tenemos un grupo de máquinas que va a trabajar a una determinada altura, Debemos considerar  que si la altitud del lugar de operación es mayor a 1,500 msnm se"]
["debe preparar el equipo para trabajos en altura, es decir \"pedir los repuestos\" necesarios para la instalación del sistema de arranque en frío. Si va a una altura"]
["inferior a 1,500 \"No considerar\"."]

{"sheet":"Hoja2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Hoja3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}