{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Hoja1","Hoja2","Hoja3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Hoja1","index":0,"n_rows":14,"n_cols":10,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Eficiencia",0.9,"x 100%",null,null,"horas trabajadas por dia",null,8]
[null,"Utilizacion",0.85,"x 100%",null,null,"dias trabajados por semana",null,5]
[null,"Demanda",10000,"unidades mensuales",null,null,null,"tiempo total",9600,"min"]
[]
["Actividad","Tiempo Estándar\n(min/Pieza)","Cantidad","TE Linea","TE Linea Ajustado","CAD Requerido","N puesto","N ajustado"]
["Corte Delantero",3.56,2,7.12,9.3071895424836608,0.96,9.6949891067538143,{"$f":"ROUNDUP(G7,0)","v":10}]
["Union Cinta Cuello",0.53,2,1.06,1.3856209150326797,0.96,1.443355119825708,{"$f":"ROUNDUP(G8,0)","v":2}]
["Trazar y Cortar Mangas",2.25,1,2.25,2.9411764705882351,0.96,3.0637254901960782,{"$f":"ROUNDUP(G9,0)","v":4}]
["Cosido de Mangas con cintas",3.46,1,3.46,4.522875816993464,0.96,4.7113289760348582,{"$f":"ROUNDUP(G10,0)","v":5}]
["Union de Mangas con Cuerpo",1.22,1,1.22,1.5947712418300652,0.96,1.6612200435729847,{"$f":"ROUNDUP(G11,0)","v":2}]
["Inspeccion de Corte y Basta",0.42,1,0.42,0.54901960784313719,0.96,0.57189542483660127,{"$f":"ROUNDUP(G12,0)","v":1}]
["Cosido de Basta",3.23,1,3.23,4.2222222222222223,0.96,4.3981481481481488,{"$f":"ROUNDUP(G13,0)","v":5}]
[null,null,null,null,null,null,null,29]

{"sheet":"Hoja2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Hoja3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}