{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Hoja1","Hoja2","Hoja3"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Hoja1","index":0,"n_rows":14,"n_cols":3,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[]
["Ejemplo"]
["Resistencias","Paralalelo","Serie"]
["R1",7,2]
["R2",11,5]
["R3",3,9]
[null,{"$f":"Resistencia_Equivalente(B4,B5,B6,2)","v":1.7633587786259541},{"$f":"Resistencia_Equivalente(C4,C5,C6,1)","v":16}]
[]
[]
["Tipo"]
["Serie",1]
["Paralelo",2]
[]
["Obs: Para el caso de calculo para dos resistencias digite el numero cero en la resistencia que no se utilizara "]

{"sheet":"Hoja2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Hoja3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}